{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":5,"rows_kept":9,"merged":[[0,0,0,4],[1,3,1,4],[4,0,4,2],[6,0,6,4]],"flags":["formulas_cached_only"]}
["全费用综合报价清单"]
[{"$nulls":3},"日期：          年    月    日"]
["序号","项目名称","工程内容","费用（元）","备注"]
[1,"泰山路（新都路-赣江路）大修工程探地雷达检测项目","  泰山路（新都路-赣江路）大修工程道路全长约3KM，对现状15米宽混合车道进行大修。根据设计图纸，在新建18cmC25水泥混凝土后采用探地雷达对混凝土板块以下路基进行检测，检测存在空洞、脱空、严重疏松、一般疏松的病害体的位置，在改性地聚合物注浆加固处理完成后采用探地雷达进行复测直至合格为止。"]
["合  计"]
[]
["注：上述费用包括完成本次招标全部内容检测人工费、检测设备设施费、组织及技术措施项目费、其他项目费、规费、税金及一定的风险费。"]
["投标人（盖章）:",null,null,"联系人："]
["法定代表人（签字或盖章）:",null,null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}